AXIOMTEK SBC Board Library Document
===================================
SBC Board : SBC87887
Wrote by  : Ray Chiang
Target : Desktop Windows
=========================
1. origional release 3.0.1.1
	uses 3.x.x.x Driver and Library
	Date : 2015-11-25
	Functions: Hardware Monitor, Watch Dog Timer, Digital IO

2. This system supports one (6 input and 2 output) with isolated

3. When the output is set to high (1), the actual output is  low voltage
   When the output is set to low  (0), the actual output is high voltage